-- name of packet
BURST events (LAYOUT 3)
[PacketHeader]
-- file in cui e' presente la descrizione dell'header
headerESATM.header
[DataFieldHeader]
-- field 0
Spare
6
none
-- field 1
Checksum flag
2
none
-- field 2
Packet Type
4
none
-- field 3
Packet subtype
4
none
-- field 4
Time Tag second (MSB)
16
none
-- field 5
Time Tag second (LSB)
16
none
-- field 6
Time Tag millisecond
16
none
-- field 7
Spare
12
none
-- field 8
Nevents
4
none
[SourceDataField]
block
variable
--type of number of block: fixed = number of block fixed equals to max number of block (fixed | variable)
variable
--supposed number (or max number) of block
79
--index of field in the [DataFieldHeader] section wich rappresent the number of event (the number of block) of the packet
8
-- offset to be added to the value given by the field m of the Data Field Header in order to obtain the correct value of the number of blocks 
0
[SourceDataFieldBlockFixed]
-- number (or max number) of element
32
-- index of field in the [SourceDataFieldBlockFixed] section wich rappresent the number of element (the number of bar) of the block
2
-- valore da sommare per ottenere il numero di element reali
1
-- field 0
1
1
none
-- field 1
spare
10
none
-- field 2
Number of bars - 1
5
none
-- field 3
TE Internal Counter (MSB)
16
none
-- field 4
TE Internal Counter (LSB)
16
none
[SourceDataFieldBlockVariable]
-- field 0
0
1
0
-- field 1
0
1
0
-- field 2
Bar ID (2 MSB)
2
none
-- field 3
PDA PHA (12 bits)
12
none
-- field 4
0
1
0
-- field 5
Bar ID (3 LSB)
3
none
-- field 6
PDB PHA (12 bits)
12
none
[Identifiers]
-- id0 APID
-- field number
3
-- type (0 header, 1 data field)
0
-- value
1294
--id1 type
2
1
15
--id2 subtype
3
1
3
