-- name of packet - CTA Triggered Sim Telescope 50 samples
triggered_telescope1_50GEN
[PacketHeader]
-- file that contains the description of the header
CTAHeaderGEN.header
[DataFieldHeader]
-- field 0
LTtime
16
none
-- field 0
LTtime__2
16
none
-- field 1
LTtime__3
16
none
-- field 2
LTtime__4
16
none
-- field 3
ArrayID
16
none
-- field 4
runNumber
16
none
[SourceDataField]
-- type of packet: noblock, block, rblock (with recoursive block)
rblock
[RBlock Configuration]
-- fixed part present (yes | no)
yes
-- variable part present (yes | no). If yes, add [RBlockX] sections.
yes
--number of rblock (if variable part is present)
2
[Fixed Part]
-- field 0
eventNumber
16
none
-- field 1
eventNumber__2
16
none
-- field 2
TelescopeID
16
none
-- field 3
numberOfTriggeredTelescopes
8
none
-- field 4
telescopeCounter
8
none
-- field 5
Number of pixels
16
none
-- field 6
Number of samples
16
none
-- field 7
Number of pixels ID zero-suppressed
16
none
[RBlock1]
--type of number of blocks of this variable part: fixed = number of block fixed equals to max number of block (fixed | variable)
variable
--number of blocks for fixed value into variable part, max number of blocks for variable value into variable part
1900
-- for variable block, number of level of headers in which is present the field with the number of blocks of the variable part (0: fixed part)
0
-- for variable block, index of field of the header which rappresent the number of events (the number of blocks) of the packet
5
-- for variable block, value to sum to get the real number of events (blocks)
0
triggered_telescope_pixel1_50GEN.rblock
[RBlock2]
--type of number of blocks of this variable part: fixed = number of block fixed equals to max number of block (fixed | variable)
variable
--number of blocks for fixed value into variable part, max number of blocks for variable value into variable part
1900
-- for variable block, number of level of headers in which is present the field with the number of blocks of the variable part (0: fixed part)
0
-- for variable block, index of field of the header which rappresent the number of events (the number of blocks) of the packet
7
-- for variable block, value to sum to get the real number of events (blocks)
0
triggered_telescope_pixelIDGEN.rblock
[Identifiers]
-- ID0
-- field number
9
-- type (0 header, 1 data field, 2 source data field)
0
-- value
1
-- ID1
-- field number
10
-- type (0 header, 1 data field, 2 source data field)
0
-- value
50
[Tail]
-- field 0
CRC
16
none
[Compression]
11
0
12
0
